
Underlay PUR 1.0 for ROCKO Flooring by Kronospan



**Material**

[PET film + polyurethane heavy-duty layer + non-woven material](https://kronoflooring-accessories.com/taxonomy/term/35)

**Width**

1.0 m

**Length**

10 m

**Thickness**

1.0 mm

**Item No. [Customer Code]**

98535 [EX PUR1.0\_SPC]

**Thermal resistance**

0,007 ㎡ K/W

**Walking sound reduction**

13%

**Impact sound reduction**

11-15 dB

**Durability**

> 1000 kPa

**Dynamic load**

> 3.000.000 Cycles

**Unevenness smoothing**

0.2 mm

**Moisture protection**

-

**Suitable for**

[](https://kronoflooring-accessories.com/taxonomy/term/26) [](https://kronoflooring-accessories.com/taxonomy/term/27) [](https://kronoflooring-accessories.com/taxonomy/term/28) [](https://kronoflooring-accessories.com/taxonomy/term/29) [](https://kronoflooring-accessories.com/taxonomy/term/64)

1 mm thick acoustic underlay specifically designed for floating floors, also suitable for laminate, cork and parquet flooring.